REMOVAL

1.Remove the engine under cover. Refer to Removal and Installation. (Procedure for VIN <JN1AR54M99M 220041/JN1AR54F79M 252231 only)

2.Remove the clip connecting the front under cover and the fender protector (LH/RH) (front). Refer to Exploded View.

3.Remove the bolt (front under cover rear edge) tightened together with the floor under cover.

4.Remove hole cover (engine under cover rear edge).(Procedure for VIN>JN1AR54M99M 220041/JN1AR54F79M 252231 only)

5.Remove the bolts (front under cover front edge) connecting the radiator core support.

6.Remove the front under cover.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Visually check the clips for deformation and damage at installation. Replace with new ones if necessary.
- Always tighten the mounting bolts to the specified torque.