■ CAUTION ■ Be careful of the following items because the range sensor is an important device to detect the shift lever position.

- Keep range sensor (A) away from magnetic cards and magnetic objects during work.
- For a person with an electro-medical apparatus, keep the range sensor away from the device.
- Keep foreign objects away from the opening (B) of range sensor during work.
- Never touch the range sensor and sensor mounting screw.
- Always shift the shift lever to the P position during work.

REMOVAL

1.Shift the shift lever to the P position.

2.Lower the rear side of the knob cover (1) downward.

3.Pull out the lock pin (2) from the shift lever knob (3).

4.Remove the shift lever knob and the knob cover.

5.Remove the console finisher assembly, instrument side panel LH/RH, and center console assembly. Refer to Exploded View.

6.Disconnect the control cable from the A/T shift selector assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

7.Disconnect the push-button ignition switch connector and the range sensor connector, and remove the harness clip.

8.Remove the A/T shift selector assembly mounting bolt.

9.Remove the A/T shift selector assembly from the vehicle.
■ CAUTION ■
Never place the A/T shift selector assembly upside-down after removal. In addition, never place the range sensor side down.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Refer to “ADJUSTMENT” in Inspection and Adjustment when installing the control cable to the A/T shift selector assembly.
- Note the following items when installing the shift lever knob.

1. Install the lock pin (1) to the shift lever knob (2).
2. Install the knob cover (3) to the shift lever knob.
3. Insert the shift lever knob into the shift lever until it clicks.