1. | Drive pinion lock nut | 2. | Companion flange | 3. | Front oil seal
4. | Pinion front bearing | 5. | Drive pinion bearing adjusting washer | 6. | Drive pinion adjusting washer
7. | Gear carrier | 8. | Pinion rear bearing | 9. | Pinion height adjusting washer
10. | Drive pinion | 11. | Drive gear | 12. | Side oil seal (right side)
13. | Side retainer | 14. | O-ring | 15. | Side bearing adjusting shim
16. | Side bearing | 17. | Differential case | 18. | Breather connector
19. | Dowel pin | 20. | Filler plug | 21. | Drain plug
22. | Gasket | 23. | Carrier cover | 24. | Gear oil defense
25. | Gasket | 26. | Side gear thrust washer | 27. | Side gear
28. | Circular clip | 29. | Pinion mate thrust washer | 30. | Pinion mate gear
31. | Pinion mate shaft | 32. | Lock pin | 33. | Side bearing adjusting washer
34. | O-ring | 35. | Side oil seal (left side) | 36. | O-ring
37. | Side shaft bearing | 38. | Extension tube retainer | 39. | Side shaft oil seal
40. | Dust seal | 41. | Side shaft |  |
A: | Oil seal lip | B: | Screw hole |  |
: Apply gear oil. Refer to Fluids and Lubricants.
: Apply anti-corrosion oil.
: Apply Genuine Medium Strength Thread Locking Sealant or equivalent. Refer to Recommended Chemical Products and Sealants.
Refer to Components for symbols not described above.