The information and specifications below apply only when engaging in performance driving.

- Before driving, check the fluid levels and adjust as necessary using the specified fluid.
- NISSAN recommends to adjust the engine oil level to be 0.39 in (10 mm) below the H mark on the engine oil dipstick. Before checking the oil level, run the engine until it reaches operating temperature and wait at least 5 minutes after turning off the engine. Make sure the oil level always remains above the L mark.
- Adjust the amount of fluid for the power steering. Refer to Inspection.
- Be sure to change the fluids listed below with the specified fluids after driving.
- Fluids temperature can be checked on the multi function display.

- Engine Coolant Temperature
- Engine Oil Temperature
- Transmission Oil Temperature

See the separate Multi Function Display Owner’s Manual.

ITEMS | GT-R SPECIFIED FLUIDS
Engine oil | Mobil 1 (0W-40)*1
Transmission oil | Genuine NISSAN Transmission Oil R35 Special*1
Differential oil (front and rear) | Castrol SAF-XJ 75W-140*1
Brake fluid | Genuine NISSAN Brake Fluid R35 Special II*1
*1: For further details, refer to Fluids and Lubricants

ENGINE OIL

- When the oil temperature stays 230°F (110°C) or below while driving:Change engine oil and engine oil filter at the same interval as Schedule 1 and 2.
- When the oil temperature reaches 230°F (110°C) up to 266°F (130°C) while driving:Change engine oil and engine oil filter every 3,100 miles (5,000 km).
- When the oil temperature exceeds 266°F (130°C) while driving:Change engine oil and engine oil filter immediately after stopping.

Check that engine oil tenperature history is not stored in ECM. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
TRANSMISSION OIL

- When the oil temperature stays 248°F (120°C) or below while driving:Change transmission oil at the same interval as Schedule 1 and 2.
- When the oil temperature reaches 248°F (120°C) up to 284°F (140°C) while driving:Change transmission oil every 3,100 miles (5,000 km).
- When the oil temperature exceeds 284°F (140°C) while driving:Change both transmission oil and differential oil immediately after stopping. Differential oil temperature usually increases concurrently.

DIFFERENTIAL OIL (FRONT AND REAR)

- When the oil temperature stays 248°F (120°C) or below while driving:Change differential oil at the same interval as Schedule 1 and 2.
- When the oil temperature reaches 248°F (120°C) up to 284°F (140°C) while driving:Change differential oil every 3,100 miles (5,000 km).
- When the oil temperature exceeds 284°F (140°C) while driving:Change both transmission oil and differential oil immediately after stopping. Differential oil temperature usually increases concurrently.

BRAKE FLUIED
Change brake fluid every 3,000 miles (5,000 km).