REMOVAL

1.Remove the front seat assembly (LH/RH). Refer to Removal and Installation.

2.Remove rear seat cushion. Refer to Removal and Installation.

3.Remove the footrest.

4.Disengage and remove the clips of floor carpet hook (1) using the remover tool (A).

| : Clip

5.Remove the floor side anchor bolt of front seat belt (LH/RH). Refer to Removal and Installation.

6.Remove the center console assembly. Refer to Removal and Installation.

7.Remove the side instrument panel (LH/RH). Refer to Removal and Installation.

8.Remove the foot duct (LH/RH) (1) and floor harness fixing clamp (B) using the remover tool (A).

9.Disconnect the center connector of diagnosis sensor unit. Refer to Removal and Installation.

10.Remove the dash side finisher (LH/RH), kicking plate inner (LH/RH), and body side welt (LH/RH). Refer to Removal and Installation.

11.Remove the front side of rear side finisher to obtain the space between rear side finisher and floor carpet.

12.Disengage the floor carpet fixing clip and then remove the tool box cover and the amplifier cover.

INSTALLATION
Install in the reverse order of removal.