CALIBRATION OF DECEL G SENSOR ■ CAUTION ■

- To calibrate pressure sensor, make sure to use CONSULT-III.
  (Calibration cannot be done without CONSULT-III.)
- Perform the pressure sensor calibration with the vehicle stopped.
- Never depress the brake pedal during the pressure sensor calibration.

1.PERFORM THE CALIBRATION OF PRESSURE SENSOR

1. Select “ABS”, “WORK SUPPORT” and “PRESS SEN CALIBRATION” in order with CONSULT-III.
2. Select “START”.
3. After approximately 10 seconds, select “END”.
4. Turn the ignition switch OFF, then turn it ON again.
   ■ CAUTION ■
   Always perform the above operation.

>> GO TO 2.
2.CHECK DATA MONITOR
Select “ABS”, “DATA MONITOR” and “PRESS SENSOR” in order with CONSULT-III, and check pressure sensor signal.

Condition | DATA MONITOR
Brake pedal is released | Approx. 0 bar
Brake pedal is depressed | Approx. 0 – 300 bar

Is the pressure within the specified range?
YES>>GO TO 3.
NO>>Check pressure sensor. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
3.ERASE THE SELF-DIAGNOSIS MEMORY
Erase self-diagnosis memories for “ABS” with CONSULT-III. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
Are the memories erased?
YES>>INSPECTION END
NO>>Check the items indicated by the self-diagnosis.