1.CHECK AIR PUMP

1. Turn ignition switch OFF.
2. Disconnect air pump harness connector.
3. Supply air pump terminals with battery voltage and check operation.

   AIR PUMP | Operation
   Connector | Terminals
   + | −
   E14 | 2 | 1 | Air pump operates

■ CAUTION ■

- The brush of the air pump may burn out. Be careful to perform the inspection taking a two- hour or more break from the latest activation of the air pump.
- Never apply the battery voltage to the air pump for 30 seconds or more continuously.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace air pump assembly.