- IPDM E/R operates the ignition relay when it receives an ignition switch ON signal from BCM via CAN communication.
- Turn the ignition relay OFF by pressing the push‐button ignition switch once when the vehicle speed is 4 km/h (2.5 MPH) or less.
- Turn the ignition relay OFF with the following operation when the vehicle speed is more than 4 km/h (2.5 MPH) or when an abnormal condition occurs in CAN communication from the unified meter and A/C amp.(Emergency OFF)

- Press and hold the push‐button ignition switch for 2 seconds or more.
- Press the push‐button ignition switch 3 times within 1.5 seconds.

NOTE：
The ignition relay does not turn ON for 3 seconds after emergency OFF even if the push‐button ignition switch is pressed.