The information and specifications below apply only when engaging in performance driving. For maximum cooling system performance, the coolant mixture ratio should be the combination of 30% antifreeze and 70% demineralized or distilled water. If ambient temperatures are anticipated below 5°F (-15°C), make sure a proper mixture ratio of 50% antifreeze and 50% demineralized or distilled water mix is used.
Do not add the coolant over the MAX level. This may cause coolant leaks because the pressure in the coolant circulation becomes high and a hose may be removed.
To Maximize vehicle performance, the coolant mixture ratio should be a combination of 30% antifreeze and 70% demineralized or distilled water for maximum cooling system performance regardless of ambient temperatures.