1.CHECK TIRE PRESSURE Check the for pressure of all wheels. Refer to Tire. Is the inspection result normal? YES>>GO TO 3. NO>>GO TO 2.
2.ADJUST TIRE PRESSURE
Check and adjust the tire pressure for all wheels specified to the value. Refer to Tire.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Check or replace the road wheels and tires, and adjust the tire pressures.
3.CHECK TIRE PRESSURE SIGNAL
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Within 5 minutes, use CONSULT-III “DATA MONITOR” to display the tire pressure for all wheels.
3. Check that the tire pressure is the specified value.

Check items | Condition | Displayed value
AIR PRESS FL | Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes. | Internal pressure of tires
AIR PRESS FR
AIR PRESS RR
AIR PRESS RL

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair or replace error-detected part.