DISASSEMBLY

1.Fix shaft with a vise.
■ CAUTION ■
Protect shaft when fixing with a vise using aluminum or copper plates.

2.Remove boot bands, and then remove boot from housing.

3.If plug needs to be removed, remove with a screw. (Left side)

4.Remove dust shield. (Right side)

5.Put matching marks on housing and shaft, and then pull out housing from shaft.
■ CAUTION ■
Use paint or similar substance for matching marks. Never scratch the surfaces.

6.Put matching marks (A) on the spider assembly and shaft.
■ CAUTION ■
Use paint or similar substance for matching marks. Never scratch the surfaces.

7.Remove snap ring (1), and then remove spider assembly from the shaft.

8.Remove boot from the shaft.

ASSEMBLY

1.Clean old grease on housing with paper waste.

2.Plug (1) has been removed, install a plug to housing (2) with a screw. (Left side)

3.Install dust shield to housing. (Right side)
■ CAUTION ■
Never reuse dust shield.

4.Install boot and boot bands to shaft.
■ CAUTION ■

- Wrap serration on shaft with tape (A) to protect boot from damage.
- Never reuse boot and boot band.

5.Remove the tape wrapped around the serration on shaft.

6.Install the spider assembly (1), align it with the matching marks (A) on the shaft (2) during the removal, and direct the serration mounting surface (B) to the shaft.

7.Assemble spider assembly onto shaft with snap ring (1).
■ CAUTION ■
Never reuse snap ring.

8.Apply the appropriate amount of grease to spider assembly and sliding surface.

9.Assemble the housing onto spider assembly, and apply the specified amount grease.

Grease amount | : Refer to Drive Shaft (GT-R certified NISSAN dealer).

10.Align matching marks painted when housing was removed.

11.Install the boot into grooves (indicated by “*” marks) shown in the figure.
■ CAUTION ■
If grease adheres to the boot mounting surface (indicated by “*” mark) on shaft or housing, boot may come off. Remove all grease from the surface.

Left side | Right side

12.To prevent the deformation of the boot, adjust the boot installation length (L) to the value shown below by inserting the suitable tool into the inside of boot from the large diameter side of boot and discharging inside air.

L | : Refer to Drive Shaft (GT-R certified NISSAN dealer).

■ CAUTION ■

- If the boot installation length is outside the standard, it may cause breakage of the boot.
- Be careful not to touch the inside of the boot with the tip of tool.

13.Install boot bands.
■ CAUTION ■
Never reuse boot band.

(1)Put boot band in the groove on drive shaft boot. Then fit pawls () into holes to temporary installation.
NOTE：
For the large diameter side, fit projection (A) and guide slit (B) at first.

(2)Pinch projection on the band with suitable pliers to tighten band.

(3)Insert tip of band below end of the pawl.

14.Secure housing and shaft, and then check that they are in the correct position when rotating boot. Install them with boot band when the mounting positions become incorrect.