DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1704 | LOW PRESSURE FL | Front left wheel pressure is or less 150 kPa (1.5 kg/cm2, 22 psi) | Low tire pressure
C1705 | LOW PRESSURE FR | Front right wheel pressure is or less 150 kPa (1.5 kg/cm2, 22 psi)
C1706 | LOW PRESSURE RR | Rear right wheel pressure is or less 150 kPa (1.5 kg/cm2, 22 psi)
C1707 | LOW PRESSURE RL | Rear left wheel pressure is or less 150 kPa (1.5 kg/cm2, 22 psi)
NOTE：
Specified tire pressure = 200 kPa (2.0 kg/cm2, 29 psi)

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1704”, “C1705”, “C1706”, or “C1707” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END