DTC | Items (CONSULT‐III screen terms) | Reference
U1000 | CAN COMM CIRCUIT | DTC Logic
U1010 | CONTROL UNIT (CAN) | DTC Logic
B257B | AMB TEMP SEN SHORT | DTC Logic
B257C | AMB TEMP SEN OPEN | DTC Logic
B2578 | IN CAR SENSOR SHORT | DTC Logic
B2579 | IN CAR SENSOR OPEN | DTC Logic
B2581 | EVAP TEMP SEN SHORT | DTC Logic
B2582 | EVAP TEMP SEN OPEN | DTC Logic
B2630* | SUNLOAD SEN SHORT | DTC Logic
B2631* | SUNLOAD SEN OPEN | DTC Logic
B2632 | DR AIRMIX ACTR SHORT | DTC Logic
B2633 | DR AIRMIX ACTR OPEN | DTC Logic
B2634 | PASS AIRMIX ACTR SHORT | DTC Logic
B2635 | PASS AIRMIX ACTR OPEN | DTC Logic
B2636 | DR VENT DOOR FAIL | DTC Logic
B2637 | DR B/L DOOR FAIL | DTC Logic
B2638 | DR D/F1 DOOR FAIL | DTC Logic
B2639 | DR DEF DOOR FAIL | DTC Logic
B263D | FRE DOOR FAIL | DTC Logic
B263E | 20P FRE DOOR FAIL | DTC Logic
B263F | REC DOOR FAIL | DTC Logic
B2654 | D/F2 DOOR FAIL | DTC Logic
B2655 | B/L2 DOOR FAIL | DTC Logic
*: Perform self‐diagnosis under sunshine. When performing indoors, aim a light more than 60 W at sunload sensor, otherwise self‐diagnosis indicates even though the sunload sensor is functioning normally.