REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove shock absorber. Refer to Exploded View.

3.Remove upper link and shims.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Assemble the shim while facing the rubber bushing toward the upper link side.

- Refer to Adjustment for selection of shims.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen conditions with tires on level ground.