1.CHECK GROUND CONNECTION

1. Turn ignition switch OFF.
2. Check ground connection M95. Refer to Ground Inspection in Circuit Inspection.

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair or replace ground connection.
2.CHECK INTAKE AIR TEMPERATURE SENSOR
Refer to Component Inspection (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>GO TO 3.
NO>>Replace mass air flow sensor (bank 1) (with intake air temperature sensor).
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END