DTC DETECTION LOGIC

DTC | CONSULT-III display description | DTC Detection Condition | Possible cause
B2562 | LOW VOLTAGE | When the power supply voltage to BCM remains less than 8.8 V for 120 seconds or more | Harness or connector (power supply circuit)

DTC CONFIRMATION PROCEDURE
1.DTC CONFIRMATION

1. Erase DTC.
2. Turn ignition switch OFF.
3. Perform the “Self Diagnostic Result” of CONSULT-III, when passed 120 seconds or more after the ignition switch is turned ON.

Is any DTC detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END