Unit | Description
Combination meter | Using the signals received from each unit and switch, controls the shift position indicator.
ECM | Transmits the engine speed signal to the combination meter via CAN communication.
TCM | Transmits the shift position signal (manual mode range) to the combination meter via CAN communication.
Meter control switch | Transmits the following signals to the combination meter.

- Enter switch signal

- Select switch signal