1.CHECK PADDLE SHIFTER (SHIFT-UP SWITCH) Check continuity between paddle shifter (shift-up switch) connector terminals.

Paddle shifter (shift-up switch) connector | Condition | Continuity
Connector | Terminal
M39 | 1 | 3 | The paddle shifter (shift-up switch) is pulled | Existed
Other than the above | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair or replace damaged parts.