DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P17C5 | 1st-Reverse position sensor compatibility | A DTC is set if the difference between the sleeve B1 position calculated from the 1st-Reverse position sensor 1 value and the sleeve B1 position calculated from the 1st-Reverse position sensor 2 is 6 mm or more. |

- 1st-Reverse position sensor 1
- 1st-Reverse position sensor 2
- Harness or connector
  (Open or short in the 1st-Reverse position sensor 1 circuit)
  (Open or short in the 1st-Reverse position sensor 2 circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P17C5 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.