REMOVAL

1.Park the vehicle on a level surface.

2.Remove the steering column cover. Refer to Exploded View.
NOTE：
Rotate the steering wheel until the mounting screw can be seen, and then remove the mounting screw.

3.Disconnect the harness connectors (C) and (D) from the paddle shifter.

A | : Paddle shifter (shift-down switch)
B | : Paddle shifter (shift-up switch)

4.Remove the bolt (E) and nut (F) from the paddle shifter.
NOTE：
Rotate the steering wheel until the mounting nut can be seen, and then remove the mounting nut.

5.Remove the paddle shifter from the steering column assembly.

INSTALLATION
Install in the reverse order of removal.