1.CHECK POWER DOOR LOCK OPERATION Check power door lock operation. Does door lock/unlock with door lock and unlock switch? YES>>GO TO 2. NO>>Refer to Diagnosis Procedure.
2.CHECK “AUTOMATIC LOCK/UNLOCK SELECT” SETTING IN “WORK SUPPORT”
Check “AUTOMATIC LOCK/UNLOCK SELECT” in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - DOOR LOCK).
Is the inspection result normal?
YES>>GO TO 3.
NO>>Set “AUTOMATIC LOCK/UNLOCK SELECT” in “WORK SUPPORT”.
3.CHECK “AUTOMATIC DOOR LOCK SELECT” SETTING IN “WORK SUPPORT”
Check “AUTOMATIC DOOR LOCK SELECT” in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - DOOR LOCK).
Is the inspection result normal?
YES>>GO TO 4.
NO>>Set “AUTOMATIC DOOR LOCK SELECT” in “WORK SUPPORT”.
4.CHECK “AUTOMATIC DOOR UNLOCK SELECT” SETTING IN “WORK SUPPORT”
Check “AUTOMATIC DOOR UNLOCK SELECT” in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - DOOR LOCK).
Is the inspection result normal?
YES>>GO TO 5.
NO>>Set “AUTOMATIC DOOR UNLOCK SELECT” in “WORK SUPPORT”.
5.CHECK TCM
Check TCM for DTC.
Refer to DTC Index.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace the malfunctioning parts.
6.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.