DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2842 | Shift fork "D" posiion circuit low | A DTC is set if the 3rd-5th position sensor voltage value received by TCM is less than 300 mV. |

- 3rd-5th position sensor
- TCM
- Harness or connector
  (Open or short in the 3rd-5th position sensor circuit)

DTC CONFIRMATION PROCEDURE
■ CAUTION ■

- If CONSULT-III is not available, “Diagnosis Procedure (GT-R certified NISSAN dealer)” must be performed before starting “DTC CONFIRMATION PROCEDURE”.
- If CONSULT-III is not available, never perform “DTC CONFIRMATION PROCEDURE” before completing the repair, which may cause secondary malfunction.
- Be careful of the driving speed.

1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDUR
With CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P2842 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.