1.WRITING MODE SELECTION CONSULT-III Configuration Select “CONFIGURATION” of BCM. When writing saved data>>GO TO 2. When writing manually>>GO TO 3.
2.PERFORM “WRITE CONFIGURATION ‐ Config file”
CONSULT-III Configuration
Perform “WRITE CONFIGURATION ‐ Config file”.
>>WORK END
3.PERFORM “WRITE CONFIGURATION ‐ Manual selection”
CONSULT-III Configuration

1. Select "WRITE CONFIGURATION ‐ Manual selection".
2. Identify the correct model and configuration list. Refer to Configuration list.
3. Confirm and/or change setting value for each item.
   ■ CAUTION ■
   Thoroughly read and understand the vehicle specification. Incorrect settings may result in abnormal control of ECU.
4. Select "SETTING".
   ■ CAUTION ■
   Make sure to select “SETTING” even if the indicated configuration of brand new BCM is same as the desirable configuration. If not, configuration which is set automatically by selecting vehicle model can not be memorized.
5. When "COMMAND FINISHED", select "END".

>>GO TO 4.
4.OPERATION CHECK
Confirm that each function controlled by BCM operates normally.
>>WORK END