REMOVAL

1.Remove the clip (A) from the front edge of the center mud guard.

2.Remove the screws (A) connecting the fender protector (rear).

3.Remove the bolt (A) and the screw (B) on the center mud guard lower surface.

4.Remove the clip of the fender protector (rear).

5.Remove the fender clips from wheel house arches, and then remove fender protector (rear) from wheel house.

6.Remove the screw (A) connecting the fender protector (front).

7.Remove the clips of the fender protector (front).

8.Remove the fender clips from wheel house arches, and then remove fender protector (front) from wheel house.

9.Remove the fender clips after removing the fender protector.

INSTALLATION
Install in the reverse order of removal.