■ WARNING ■

- Before servicing, turn ignition switch OFF, disconnect battery negative terminal, and wait at least 3 minutes or more. (To discharge backup capacitor.)
- Never use unspecified tester or other measuring device.

1.PERFORM COLLISION DIAGNOSIS
Perform collision diagnosis.Refer to When SRS is activated in a collision or When SRS is not activated in a collision.
Iscollision diagnosis complete?
YES>>GO TO 2.
NO>>INSPECTION END
2.FINAL INSPECTION
Perform “AIR BAG” Self Diagnostic Result.
Is the inspection result normal?
YES>>INSPECTION END
NO>>Peform diagnosis of applicable DTC.Refer to DTC Index.