TOE-IN

1.Remove rear diffuser. Refer to Exploded View.

2.Adjust using the adjust bolt (2) of rear lower link (1).

Toe-in | : Refer to Wheel Alignment.

■ CAUTION ■

- Always evenly adjust both toe-in alternately and adjust the difference between the left and right to the standard.
- Always hold the adjust bolt firmly when tightening nut.

CAMBER

1.Remove rear diffuser. Refer to Exploded View.

2.Adjust using the adjust bolt (2) of front lower link (1).

Camber | : Refer to Wheel Alignment.

■ CAUTION ■

- Always hold the adjust bolt firmly when tightening nut.
- Always check toe-in after adjusting camber.