REMOVAL ■ CAUTION ■ Use shop cloths to protect parts from damage during removal and installation.

1.Remove the seat cushion.

- Lift up the seat cushion lower side, disengage the joint by pulling the ring (1) of the cushion hook on the front bottom, and then lift up the seat cushion (2) to remove the seat cushion.
- Remove the seat cushion from the vehicle.

2.Remove the seatback.

- Remove the seatback lower mounting nut.
- Remove the seatback from the vehicle.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Use shop cloths to protect parts from damage during removal and installation.