REMOVAL

1.Remove the inner anchor.

- Remove rear seat cushion. Refer to Removal and Installation.
- Remove the inner anchor mounting anchor bolts.

2.Remove the seat belt retractor.

- Remove rear seatback. Refer to Removal and Installation.
- Remove the kicking plate inners (LH/RH), rear side finishers (LH/RH), and rear pillar finishers (LH/RH). Refer to Removal and Installation.
- Remove rear parcel shelf. Refer to Removal and Installation.
- Remove the rear seat belt escutcheon from the rear parcel shelf.
- Remove the insulator.
- Remove the mounting anchor bolts, and then remove the seat belt retractor.
- Remove the retractor cover.

INSTALLATION
Install in the reverse order of removal.