Work after rear fender is removed. ■ CAUTION ■ Create the reinforcing sheet from the redundant area of service parts for butt welding area. Weld the reinforcing sheet on the back of butt welding area, and then perform butt welding. After welding, apply anti‐corrosive wax on the reinforcing sheet‐welded area.

Unit: mm (in) |  |  |  |
: Vehicle front : Weld the parts onto the back of the component part.
Replacement parts
• | Lock pillar reinforcement (LH) |  |  |  |