OPERATION DESCRIPTION The warning function are as per the following and are given to the user as warning information and warnings using combinations of Intelligent Key warning buzzer, KEY warning lamp, key slot illumination and information display in combination meter.

- Intelligent Key system malfunction
- OFF position warning
- P position warning
- ACC warning
- Take away warning
- Door lock operation warning
- Key warning
- Intelligent Key insert information
- Engine start information
- Steering lock information
- Intelligent key low battery warning
- Key ID warning

OPERATION CONDITION
Once the following condition from below is established, alert or warning is executed.

Warning/Information functions | Operation procedure
Intelligent Key system malfunction | When a malfunction is detected on BCM, “KEY” warning lamp illuminates.
OFF position warning | For internal |

- Ignition switch: ACC position.
- Door switch (driver side): ON (Door is open).

For external | OFF position warning (For internal) is in active mode, driver side door is closed. NOTE： OFF position (For external) active only when each of the sequences occurs as below: P position warning → ACC warning → OFF position warning (For internal) → OFF position warning (For internal)
P position warning | For internal |

- Shift position: Except P position.
- Engine is running to stopped (Ignition switch is ON to OFF).

For external | Warning is activated when driver door is closed from the open position while the P position warning (for inside vehicle) is ON.
ACC warning |

- When P position warning is in active mode, shift position changes P position.
- Ignition switch: ACC position.

Take away warning | Door is open to close |

- Ignition switch: Except LOCK position.
- Door switch: ON to OFF (Door is open to close).
- Intelligent Key cannot be detected inside the vehicle.

Door is open |

- Door switch: ON (Door is open).
- Key ID verification every 5 seconds when registered Intelligent Key cannot be detected inside the vehicle.

Push button-ignition switch operation |

- Ignition switch: Except LOCK position.
- Press push-button ignition switch.
- Intelligent Key cannot be detected inside the vehicle.

Intelligent Key is removed from key slot |

- When Intelligent Key is removed from key slot.
- Intelligent Key cannot be detected inside the vehicle.
- Ignition switch: Except LOCK position.
- When intelligent Key is low battery.

Door lock operation warning | When door lock operation is requested while door lock operating condition of door request switch is not satisfied.
Key warning |

- Ignition switch is OFF position.
- Driver side door switch: ON (Driver side door is open).
- Intelligent Key is inserted in key slot.

Intelligent Key insert information |

- Door switch: ON to OFF (Door is open to close).
- Intelligent Key is out of key slot.
- Intelligent Key cannot be detected inside the vehicle.

Engine start information | Ignition switch is ON position |

- Ignition switch: ON position.
- Shift position: P position.
- Engine is stopped.

Ignition switch is except ON position |

- Ignition switch: Except ON position.
- Shift position: P position.
- Intelligent Key is inserted in key slot or Intelligent Key can be detected inside the vehicle.

Steering lock information | When steering lock cannot be released after ignition switch is turned ON.
Intelligent Key low battery warning | When Intelligent Key is low battery, BCM is detected after ignition switch is turned ON.
Key ID warning | When registered intelligent Key cannot be detected inside the vehicle after ignition switch is turned ON.

WARNING METHOD
The following table shows the alarm or warning methods with chime.
Information display (combination meter), “KEY” indicator or key slot indicator when the warning conditions are met.

Warning/Information functions | “KEY” warning lamp | Information display (combination meter) | Key slot indicator | Warning chime
Combination meter buzzer | Intelligent Key warning buzzer
Intelligent Key system malfunction | Illuminate | — | — | — | —
OFF position warning | For internal | — | — | — | Activate | —
For external | — | — | — | — | Activate
P position warning | For internal | — |  | — | Activate | —
For external | — | Activate
ACC warning | — |  | — | — | —
Take away warning | Door is open to close | — |  | Blink | Activate | Activate
Door is open | — | Blink | — | —
Push-ignition switch operation | — | Blink | Activate | —
Intelligent Key is removed from key slot | — | Blink | — | —
Door lock operation warning | Request switch operation | — | — | — | — | Activate
Intelligent Key operation | — | — | — | — | Activate
Key ID warning | — |  | — | — | —
Key warning | — |  | Blink | Activate | —
Intelligent Key insert information | — |  | Illuminate | — | —
Engine start information | — |  | — | — | —
Steering lock information | — |  | — | — | —
Intelligent Key low battery warning | — |  | — | — | —

LIST OF OPERATION RELATED PARTS
Parts marked with × are the parts related to operation.

Warning function | Intelligent Key | Key slot | Ignition switch | Door switch | Door request switch | Inside key antenna | Outside key antenna | Intelligent Key warning buzzer | Combination meter warning buzzer | CAN communication system | BCM | Combination meter display | Key slot indicator | Detention switch | “KEY” warning lamp
Intelligent Key system malfunction |  |  |  |  |  |  |  |  |  | × | × |  |  |  | ×
OFF position warning | For internal |  |  |  | × |  |  |  |  | × | × | × |  |  |  |
For external |  |  |  | × |  |  |  | × |  |  | × |  |  |  |
P position warning |  |  | × | × |  |  |  |  | × | × | × | × |  | × |
ACC warning |  |  | × |  |  |  |  |  | × | × | × | × |  | × |
Take away warning | Door is open or close | × |  |  | × |  | × |  | × | × | × | × | × | × |  |
Door is open | × |  |  | × |  | × |  |  |  | × | × | × | × |  |
Push-ignition switch operation | × |  | × |  |  | × |  |  | × | × | × | × | × |  |
Intelligent Key is removed from key slot | × | × |  |  |  | × |  |  |  | × | × | × | × |  |
Door lock operation warning | × | × |  | × | × | × | × | × |  |  | × |  |  |  |
Key ID warning | × | × | × |  |  | × |  |  |  | × | × | × |  |  |
Key warning | × | × |  | × |  |  |  |  | × | × | × | × | × |  |
Intelligent Key insert information | × | × | × | × |  | × |  |  |  | × | × | × | × |  |
Engine start information | Ignition switch is in the ON position | × | × | × |  |  | × |  |  |  | × | × | × |  | × |
Ignition switch is in any position except the ON position | × | × | × |  |  | × |  |  |  | × | × | × |  |  |
Steering lock information |  |  | × |  |  |  |  |  |  | × | × | × |  |  |
Intelligent Key low battery warning | × |  |  |  |  | × |  |  |  | × | × | × |  |  |