DTC DETECTION LOGIC

DTC | Display items | Malfunction detected condition | Possible cause
C1204 | 4WD SOLENOID | Malfunction related to AWD solenoid has been detected. | Internal malfunction of electric controlled coupling

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform self-diagnosis for “ALL MODE AWD/4WD”.

Is DTC “C1204” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END