Add the correct amount of lubricant to the system after replacing any of the following major components. Amount of lubricant to be added:

Replaced part | Lubricant to be added to system | Remarks
Amount of lubricant m (US fl oz., Imp fl oz.)
Evaporator | 75 (2.5, 2.6) | —
Condenser | 35 (1.2, 1.2) | —
Liquid tank | 10 (0.3, 0.4) | —
In case of refrigerant leakage | 30 (1.0, 1.1) | Large leakage
— | Small leakage *1
*1: No addition of lubricant is needed if the refrigerant leakage is small.