REMOVAL

1.Remove tire with power tool. Refer to Exploded View.

2.Remove rear diffuser. Refer to Exploded View.

3.Set suitable jack under rear suspension member.

4.Loosen rear suspension member mounting nuts, and gradually lower jack to rear suspension member.
■ CAUTION ■
Never remove rear suspension member mounting bolts and nuts.

5.Remove radius rod.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen conditions with tires on level ground.