REMOVAL

1.Remove instrument power socket assembly (1) by using a remover tool.

| : Pawl

2.Disconnect power socket connector (A).

2 | : Ring
D | : Cut out

3.Pull out inner socket (1) by pushing the ring pawl (B) from the inner socket hole (square) (C).

4.Remove seal (3) by pushing the ring pawl.

INSTALLATION
Install in the reverse order of removal.
NOTE：
Align the cut outs of inner socket, ring, and seal.