Unit | Description
Combination meter | Based on received signals from each unit, switch, and sensor, controls the following items.

- Speedometer

- Tachometer

- Engine coolant temperature gauge

- Fuel gauge

- Warning lamp

- Indicator lamp

- Information display

Fuel level sensor unit | Detects the fuel level in fuel tank using the fuel level sensor unit, and transmits the fuel gauge signal to the combination meter.
Oil pressure sensor | Detects the oil pressure of engine oil, and transmits the oil pressure sensor signal to the combination meter.
ECM | Transmits the following signals to the combination meter via CAN communication.

- Engine speed signal

- Engine coolant temperature signal

- Fuel consumption monitor signal

- Malfunction indicator lamp signal

- Engine status signal

- ASCD status signal

ABS actuator and electric unit (control unit) | Transmits the following signals to the combination meter via CAN communication.

- Vehicle speed signal

- ABS warning display signal

- VDC warning display signal

BCM | Transmits signals received from each unit and switch to the combination meter via CAN communication.
TCM | Transmits the following signals to the combination meter via CAN communication.

- Shift position signal

- Shift lever position warning display signal

- Transmission oil high temperature warning display signal

- Transmission clutch high temperature warning display signal

- Transmission system warning display signal

- Transmission system check display signal

- Shift lever position check display signal

AWD control unit | Transmits the following signals to the combination meter via CAN communication.

- AWD clutch high temperature warning display signal

- AWD system warning display signal

- Front/rear tire size discrepancy warning display signal

Low tire pressure warning control unit | Transmits the following signals to the combination meter via CAN communication.

- Run-flat tire warning display signal

- Low tire pressure warning display signal

- Tire pressure monitoring system warning display signal

Meter control switch | Transmits the following signals to the combination meter.

- Illumination control switch signal (+)

- Illumination control switch signal (-)

- Trip A/B reset switch signal

- Select switch signal

- Enter switch signal

Brake fluid level switch | Transmits the brake fluid level switch signal to the combination meter.
Parking brake switch | Transmits the parking brake switch signal to the combination meter.
Oil level sensor | Transmits the oil level sensor signal to the combination meter.
Washer level switch | Transmits the washer level switch signal to the combination meter.
Ambient sensor | Transmits the ambient sensor signal to the combination meter.