REMOVAL

1.Remove compressor together with low-pressure pipe 2. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove mounting nut of low‐pressure pipe 2, and then remove low-pressure pipe 2 from compressor.
■ CAUTION ■
Cap or wrap the joint of the cooler piping and compressor with suitable material such as vinyl tape to avoid the entry of air.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■

- Replace O‐rings with new ones. Then apply compressor oil to them when installing.
- Female‐side piping connection is thin and easy to deform. Slowly insert the male‐side piping straight in axial direction.
- Insert piping securely until a click is heard.
- After piping connection is completed, pull male‐side piping by hand to make sure that connection does not come loose.
- Check for leakages when recharging refrigerant.