REMOVAL Front diffuser RH

1.Remove the bolt (rear diffuser front edge) tighten together with the rear diffuser (center).

2.Remove the front diffuser RH mounting bolts.

3.Remove the front diffuser RH.

Front diffuser LH

1.Remove the bolt (rear diffuser front edge) tighten together with the rear diffuser (center).

2.Remove the front diffuser LH mounting bolts.

3.Remove the front diffuser LH.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When front diffuser mounting bolt is removed, check for surface treatment peel off and oxidation of mounting bolt and washer so that electric corrosion is prevented.
- Regarding mounting bolt and washer with surface treatment peel off, paint contact surface of washer and carbon using touch pen or others. By doing so, mounting bolt and washer are reusable. However, regarding oxidation, never reuse.
- For mounting portion of transmission mounting stay, always replace mounting bolts to new ones in order to prevent electric corrosion.
- Always tighten the mounting bolts to the specified torque.