APPLICATION ITEM CONSULT‐III performs the following functions via CAN communication with IPDM E/R.

Diagnosis mode | Description
Ecu Identification | Allows confirmation of IPDM E/R part number.
Self Diagnostic Result | Displays the diagnosis results judged by IPDM E/R.
Data Monitor | Displays the real-time input/output data from IPDM E/R input/output data.
Active Test | IPDM E/R can provide a drive signal to electronic components to check their operations.
CAN Diag Support Monitor | The results of transmit/receive diagnosis of CAN communication can be read.

SELF DIAGNOSTIC RESULT
Refer to DTC Index.
DATA MONITOR
Monitor item

Monitor Item [Unit] | MAIN SIGNALS | Description
RAD FAN REQ [%] | × | Displays the value of the cooling fan speed signal received from ECM via CAN communication.
AC COMP REQ [Off/On] | × | Displays the status of the A/C compressor request signal received from ECM via CAN communication.
TAIL&CLR REQ [Off/On] | × | Displays the status of the position light request signal received from BCM via CAN communication.
HL LO REQ [Off/On] | × | Displays the status of the low beam request signal received from BCM via CAN communication.
HL HI REQ [Off/On] | × | Displays the status of the high beam request signal received from BCM via CAN communication.
FR FOG REQ [Off/On] | × | NOTE： The item is indicated, but not monitored.
FR WIP REQ [Stop/1LOW/Low/Hi] | × | Displays the status of the front wiper request signal received from BCM via CAN communication.
WIP AUTO STOP [STOP P/ACT P] | × | Displays the status of the front wiper stop position signal judged by IPDM E/R.
WIP PROT [Off/BLOCK] | × | Displays the status of the front wiper fail-safe operation judged by IPDM E/R.
IGN RLY1 ‐REQ [Off/On] |  | Displays the status of the ignition switch ON signal received from BCM via CAN communication.
IGN RLY [Off/On] | × | Displays the status of the ignition relay judged by IPDM E/R.
PUSH SW [Off/On] |  | Displays the status of the push‐button ignition switch judged by IPDM E/R.
INTER/NP SW [Off/On] |  | Displays the status of the shift position judged by IPDM E/R.
ST RLY CONT [Off/On] |  | Displays the status of the starter relay status signal received from BCM via CAN communication.
IHBT RLY ‐REQ [Off/On] |  | Displays the status of the starter control relay signal received from BCM via CAN communication.
ST/INHI RLY [Off/ ST ON/INHI ON/UNKWN] |  | Displays the status of the starter relay and starter control relay judged by IPDM E/R.
DETENT SW [Off/On] |  | Displays the status of the control device (detention switch) judged by IPDM E/R.
S/L RLY ‐REQ [Off/On] |  | Displays the status of the steering lock relay request signal received from BCM via CAN communication.
S/L STATE [LOCK/UNLOCK/UNKWN] |  | Displays the status of the steering lock judged by IPDM E/R.
DTRL REQ [Off/On] | × | Displays the status of the daytime running light request signal received from BCM via CAN communication. NOTE： This item is monitored only the vehicle with daytime running light system.
OIL P SW [Open/Close] |  | NOTE： The item is indicated, but not monitored.
HOOD SW [Off/On] |  | Displays the status of the hood switch judged by IPDM E/R.
HL WASHER REQ [Off/On] |  | NOTE： The item is indicated, but not monitored.
THFT HRN REQ [Off/On] |  | Displays the status of the theft warning horn request signal received from BCM via CAN communication.
HORN CHIRP [Off/On] |  | Displays the status of the horn reminder signal received from BCM via CAN communication.
CRNRNG LMP REQ [Off/On] |  | NOTE： The item is indicated, but not monitored.

ACTIVE TEST
Test item

Test item | Operation | Description
CORNERING LAMP | Off | NOTE： The item is indicated, but cannot be tested.
LH
RH
HORN | On | Operates horn relay 1 and horn relay 2 for 20 ms.
FRONT WIPER | Off | OFF
Lo | Operates the front wiper relay.
Hi | Operates the front wiper relay and front wiper high relay.
MOTOR FAN | 1 | OFF
2 | Outputs 50% pulse duty signal (PWM signal) to the cooling fan control module.
3 | Outputs 80% pulse duty signal (PWM signal) to the cooling fan control module.
4 | Outputs 100% pulse duty signal (PWM signal) to the cooling fan control module.
HEAD LAMP WASHER | On | NOTE： The item is indicated, but cannot be tested.
EXTERNAL LAMPS | Off | OFF
TAIL | Operates the tail lamp relay.
Lo | Operates the headlamp low relay.
Hi | Operates the headlamp low relay and ON/OFF the headlamp high relay at 1 second intervals.
Fog | NOTE： The item is indicated, but cannot be tested.