1.CHECK POWER SUPPLY

1. Turn ignition switch OFF.
2. Disconnect auto anti-dazzling inside mirror (homelink universal transceiver) connector.
3. Check voltage between auto anti-dazzling inside mirror (home link universal transceiver) harness connector and ground.

(+) | (-) | Condition | Voltage (V) (Approx.)
Auto anti-dazzling inside mirror (Homelink universal transceiver)
connector | Terminal | Ground | Ignition switch position | OFF | Battery voltage
R9 | 5 | ON

Is the inspection result normal?
YES>>GO TO 2.
NO-1>>10A fuse [No. 6 located in the fuse block (J/B)].
NO-2>>Harness for open or short between fuse and auto anti-dazzling inside mirror (homelink universal transceiver).
2.CHECK GROUND CIRCUIT
Check continuity between auto anti-dazzling inside mirror (homelink universal transceiver) harness connector and ground.

Auto anti-dazzling inside mirror (Homelink universal transceiver) | Ground | Continuity
Connector | Terminal
R9 | 8 | Existed

Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair harness.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END