1.CHECK TPMS Check the status of the low tire pressure warning lamp for illumination. Is the low tire pressure warning lamp illuminated? YES>>Check the power supply and ground circuit. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>GO TO 2.
2.CHECK TRANSMITTER ID REGISTRATION
With CONSULT-III
Perform the self-diagnosis of the low tire pressure warning control unit.
Is any malfunction detected?
YES>>Check malfunctioning circuit.
NO>>GO TO 3.
3.CHECK LOW TIRE PRESSURE WARNING LAMP
Perform trouble diagnosis of the low tire pressure warning lamp. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>Check pin terminal and connection of each connector for damage and loose connection.
NO>>Repair or replace error-detected parts.