REMOVAL

1.Remove high-pressure pipe 2. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove mounting nuts (A), and then remove cowl top reinforcement (1).

3.Remove low‐pressure flexible hose.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■

- Replace O‐rings with new ones. Then apply compressor oil to them when installing.
- Female‐side piping connection is thin and easy to deform. Slowly insert the male‐side piping straight in axial direction.
- Insert piping securely until a click is heard.
- After piping connection is completed, pull male‐side piping by hand to make sure that connection does not come loose.
- Check for leakages when recharging refrigerant.