1. | Mechanical key | 2. | Upper case | 3. | Switch rubber
4. | Circuit board | 5. | Battery | 6. | Lower case

1.Unlock the lock knob on the rear of Intelligent Key, and then remove the mechanical key.

2.Insert a screwdriver wrapped with tape into Area A and then separate lower and upper cases by twisting screwdriver.

3.When replacing the battery with new oneRemove the battery from the lower half of the case and replace it.

Battery replacement | :Coin-shaped lithium battery 3 V (CR2032)

■ CAUTION ■
Keep dirt, grease, and other foreign matter off the electrode contact area when replacing battery.

4.Remove circuit board assembly from upper case. (Substrate assembly: circuit board + switch rubber)

5.When replacing the circuit board or switch rubberGently press the switch rubber and remove the circuit board.
■ CAUTION ■
Never touch the printed circuits directly.

6.After replacement, assemble the upper and lower cases by engaging the hooks on their circumference while being careful not to pinch the switch rubber, etc.
■ CAUTION ■

- After replacing the battery, check that all Intelligent Key functions work normally.