REMOVAL Driver Side

1.Remove instrument panel pad A. Refer to Exploded View.

2.Pull to remove center ventilator grille (1) and side ventilator grille (2) from instrument panel pad A (3), using flat screwdriver to push the pawls.

| : Pawl

Passenger Side

1.Remove instrument panel pad C. Refer to Exploded View.

2.Pull to remove center ventilator grille (1) and side ventilator grille (2) from instrument panel pad C (3), using flat screwdriver to push the pawls.

| : Pawl

INSTALLATION
Installation is basically the reverse order of removal.