DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0979 | Shift solenoid "C" control circuit low | A DTC is set if the shift solenoid valve 3 monitor value is OFF when the shift solenoid valve 3 command value is ON. |

- Shift solenoid valve 3
- Harness or connector
  (Open or short in the shift solenoid valve 3 circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Shift the shift lever to the R position and run at idle for 5 seconds or more.
3. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Shift the shift lever to the R position and run at idle for 5 seconds or more.
3. Check self-diagnosis.

Is DTC P0979 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.