DISASSEMBLY

1.Rotate the resin cap counterclockwise and unlock it.

2.Rotate the xenon bulb socket counterclockwise and unlock it.

3.Remove the retaining spring lock. And then remove the xenon bulb.

4.Remove the HID control unit installation screw.

5.Remove the HID control unit harness installation screw. And then disconnect the connector from HID control unit.

6.Pull out the xenon bulb socket from the headlamp housing assembly.

7.Rotate the resin cap counterclockwise and unlock it.

8.Disconnect the headlamp (HI) connector.

9.Rotate the halogen bulb socket counterclockwise and unlock it.

10.Remove the halogen bulb socket from the headlamp housing assembly.

11.Rotate the parking lamp bulb socket counterclockwise and unlock it.

12.Remove the bulb from the parking lamp bulb socket.

13.Rotate the front turn signal lamp bulb socket counterclockwise and unlock it.

14.Remove the bulb from the front turn signal lamp bulb socket.

ASSEMBLY
Assemble in the reverse order of disassembly.
■ CAUTION ■

- Install HID control unit securely.
- After installing the bulb, install the resin cap and the bulb socket securely for watertightness.
- Seal packing cannot be reused.
- After installation, check that headlamp lighting. Refer to Inspection After Installation (HID Control Unit).