REMOVAL

1.Remove the clip (A)

| : Vehicle front

2.Pull out the washer tank inlet from the washer tank.

3.Remove the front bumper fascia. Refer to Exploded View.

4.Disconnect the washer pump connector.

5.Disconnect the washer level switch connector.

6.Disconnect the front washer tube.

7.Remove the washer tank mounting bolts.

8.Remove the washer tank from the vehicle.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Add water up to the top of the washer tank inlet after installing. Check that there in no leakage.