1.INSPECTION START

1. Turn ignition switch ON.
2. Check “Self diagnostic result” with CONSULT-III.
3. Touch “ERASE”.
4. Perform DTC Confirmation Procedure.Refer to DTC Logic.

Is the DTC B26E9 displayed again?
YES>>GO TO 2.
NO>>GO TO 3.
2.REPLACE STEERING LOCK UNIT

1. Replace steering lock unit.
2. Perform DTC confirmation procedure. Refer to DTC Logic.

Is the DTC B26E9 displayed again?
YES>>GO TO 3.
NO>>INSPECTION END
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END