DTC DETECTION LOGIC

DTC | CONSULT‐III display description | DTC Detection Condition | Probable cause
B26E7 | TPMS CAN COMM | When ignition switch is ON, BCM cannot received CAN communication signal from low tire pressure warning control unit. |

- CAN communication system
- Low tire pressure warning control unit
- BCM

DTC CONFIRMATION PROCEDURE
1.DTC CONFIRMATION

1. Erase the DTC.
2. Turn ignition switch OFF.
3. Perform the “Self Diagnostic Result” of CONSULT-III, when passed 2 seconds or more after the ignition switch is turned ON.

Is any DTC detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END