1.BRAKE WARNING LAMP OPERATION CHECK 1 Check that the lamp illuminates for approximately 2 seconds after the ignition switch is turned ON. Is the inspection result normal? YES>>GO TO 2. NO>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.BRAKE WARNING LAMP OPERATION CHECK 2
Check that the brake warning lamp in the combination meter turns ON/OFF correctly when operating the parking brake pedal.
Is the inspection result normal?
YES>>INSPECTION END
NO>>Check parking brake switch. Refer to Diagnosis Procedure.