1.BRAKE WARNING LAMP OPERATION CHECK

1. Start the engine.
2. Operate the parking brake, then check the illumination status of brake warning lamp.

Parking brake applied | :ON
Parking brake released | :OFF

Is the inspection result normal?
YES>>Replace the combination meter.
NO>>GO TO 2.
2.CHECK PARKING BRAKE SWITCH SIGNAL CIRCUIT
Perform the parking brake switch signal circuit inspection. Refer to Diagnosis Procedure.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair the harnesses or connectors.
3.CHECK PARKING BRAKE SWITCH
Perform the unit inspection of parking brake switch. Refer to Component Inspection.
Is the inspection result normal?
YES>>Replace the combination meter.
NO>>Replace the parking brake switch.